# Заявка на подключение Stream

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | | | E-Health2 \_2 | |
| VPN gateway NATed (YES/NO)? | | | NO | |
| Public IP address of VPN gateway (Peer IP) | | | 80.255.70.84 | |
| Key | | | 1tYhpQlr0v | |
| IKE Phase1 | | | | | |
| Authentication: | | | pre-share key | |
| Hash: (SHA-1 или MD5) | | | SHA-1 | |
| Encryption: (AES (256 Bits), AES (128 Bits), 3DES) | | | 3DES | |
| Diffie-Hellman group: | | | Group 2 (1024) | |
| IKE mode: | | | main | |
| Lifetime: | | | 86400 sec | |
| IKE Phase2 (transform-set) | | | | | |
| IPSec Mode: | | | Tunnel | |
| Encryption: (AES (256 Bits), AES (128 Bits), 3DES) | | | AES-128 | |
| Perfect Forward Secrecy (PFS):  (NO или YES, DH group) | | | No | |
| Hash: | | | SHA-1 | |
| Lifetime: | | | 3600 (can be different, tunnel just reestablishes from time to time. Possible to set per ipsec policy) | |
| Lifetime kilobytes: | | | 1843200 (can be different, tunnel just reestablishes from time to time. Possible to set per ipsec policy) | |
| List of hosts, involved in VPN-connection. | | | | | | | |
| №№ | Stream | | |  | | | |
| Original IP | Translated IP | | Translated IP | | | Original IP |
| 1 | 35.190.207.42 | 172.25.63.156 | | 172.25.60.131 | | | SMPP server |
| 2 |  |  | |  | | |  |
| 3 |  |  | |  | | |  |
| 4 |  |  | |  | | |  |
| ACL | | | | | | | |
| №№ | Source | | Destination | | | | Service (Port) |
| 1 | 172.25.63.156 | | 172.25.60.131 | | | | 8313 |
| 2 |  | |  | | | |  |
| 3 |  | |  | | | |  |

Login: 003355

Password in sms: Уважаемый XXXXXXX пользователь

Cервис "Процессинговые рассылки" активирован. Для его использования воспользуйтесь параметрами:

Логин:

Пароль: